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Grade 10: _______________ 		Student Name:_______________

LC4- Lesson 21
Computer Hardware

True/False
Indicate whether the statement is true or false.

____	1.	After the control unit sends out messages to execute instructions, it changes those instructions into machine language.

____	2.	When a switch contains electricity, it represents a zero.

____	3.	The processor is the "brains" of the computer.

____	4.	The memory on the motherboard is short term.

____	5.	RAM is volatile.

____	6.	A machine cycle cannot contain more than one execution cycle.

____	7.	ROM is volatile.

____	8.	A motherboard can contain more than one controller.

____	9.	The joystick is the most common input device for entering numeric and alphanumeric data.

____	10.	Optical storage devices use laser technology to read and write data.

____	11.	A mouse must be connected to the computer with a cable or cord.

____	12.	You can use vocal commands if a computer has a voice recognition device.

____	13.	A trackball is an output device.

____	14.	The resolution of a monitor is measured in the number of pixels or dots that it can display.

____	15.	Storage devices are categorized by the amount of data they can store.


Multiple Choice
Identify the choice that best completes the statement or answers the question.

____	16.	Which is not a part of IPOS?
	a.
	information
	c.
	output

	b.
	storage
	d.
	input




____	17.	The ____ is central to the computer system.
	a.
	system board
	c.
	component case

	b.
	motherboard
	d.
	system case




____	18.	When a switch does not contain electricity, it represents a ____.
	a.
	3
	c.
	1

	b.
	0
	d.
	2




____	19.	____ are special instructions that control the activities of a computer.
	a.
	CPUs
	c.
	Programs

	b.
	Chips
	d.
	ALUs




____	20.	Machine language is also known as ____.
	a.
	control language
	c.
	CPU

	b.
	BASIC
	d.
	binary




____	21.	Short term memory is also known as ____.
	a.
	FRM
	c.
	RAM

	b.
	CPU
	d.
	DRAM




____	22.	The more ____ that your computer has, the faster it processes data.
	a.
	RAM
	c.
	PICO

	b.
	CPU
	d.
	NANOS




____	23.	The ____ cycle refers to the amount of time it takes a CPU to execute an instruction and store the results.
	a.
	machine
	c.
	system

	b.
	instruction
	d.
	execution




____	24.	The computer manufacturer uses ____ to store specific instructions that are needed for computer operations.
	a.
	RAM
	c.
	CPU

	b.
	ROM
	d.
	SYS



____	25.	Which accurately describes a controller?
	a.
	It controls the RAM, which allows you to measure machine cycles.

	b.
	It controls data on the ROM.

	c.
	It controls the transfer of data from a computer to a peripheral device.

	d.
	It is measured in pico seconds.



____	26.	Which number would you find in binary code?
	a.
	1
	c.
	2

	b.
	–1
	d.
	22



____	27.	A ____ is a device that controls the transfer of data from the computer to a peripheral device or vice versa. 
	a.
	controller
	c.
	plotter

	b.
	motherboard
	d.
	mouse




____	28.	A(n) ____ device enables you to enter data into and issue commands to a computer.
	a.
	controller
	c.
	output

	b.
	memory
	d.
	input



____	29.	Which of the following is NOT an output device?
	a.
	monitor
	c.
	printer

	b.
	scanner
	d.
	speaker



____	30.	A ____ is an example of an optical storage device.
	a.
	CD-ROM
	c.
	Jaz drive

	b.
	floppy diskette
	d.
	network drive



Completion
Complete each statement.
	eight
	circuit
	arithmetic
	cards
	motherboard

	expansion slot
	control
	cycle
	machine
	ASCII

	printer
	hard disk drive

	modem
	function
	clicking

	Arrow
	magnetic scanner
	pointer
	laser
	magnetic tape drive




	31.	The motherboard is a(n) ____________________ board.

	32.	The CPU has two primary sections: the control unit and the ____________________/logic unit.

	33.	The ____________________ unit coordinates all activities from the CPU.

	34.	The faster the ____________________ cycle, the faster your computer processes data.

	35.	An instruction ____________________ is the amount of time it takes to retrieve an instruction and complete the respective command.

	36.	Expansion boards are also called expansion ____________________.

	37.	Expansion slots are located on the ____________________.

	38.	The most popular code system is ________________________________________.

	39.	A byte comprises ____________________ bits.

	40.	A(n) ____________________ is an opening on the motherboard where a circuit board can be inserted.

	41.	The ____________________ is an example of a device that can perform both input and output functions.

	42.	The _____________________ keys on the keyboard are used to give the computer commands.

	43.	Pressing and releasing the mouse button is referred to as ____________________.

	44.	A(n) ______________________ produces a hard copy of processing results.

	45.	A(n) ____________________ is a type of storage media used to store large amounts of data inside the computer.

	46.	____________________ keys allow you to move the position of the cursor on the screen.

	47.	The ____________________ is an on-screen object that you move with the mouse to select text and access commands.

	48.	A(n) __________________________ reads encoded information on the back of a credit card.

	49.	A(n) _____________________ printer produces high-quality images using a powder substance called toner.

	50.	A type of storage device often used to back up large volumes of data is a(n) _________________________.

Answer Section

TRUE/FALSE

	1.	ANS:	T	PTS:	1	REF:	22

	2.	ANS:	F	PTS:	1	REF:	22

	3.	ANS:	T	PTS:	1	REF:	21

	4.	ANS:	T	PTS:	1	REF:	23

	5.	ANS:	T	PTS:	1	REF:	23

	6.	ANS:	F	PTS:	1	REF:	24

	7.	ANS:	F	PTS:	1	REF:	25

	8.	ANS:	T	PTS:	1	REF:	22

	9.	ANS:	F	PTS:	1	REF:	26

	10.	ANS:	T	PTS:	1	REF:	36

	11.	ANS:	F	PTS:	1	REF:	27

	12.	ANS:	T	PTS:	1	REF:	28

	13.	ANS:	F	PTS:	1	REF:	30

	14.	ANS:	T	PTS:	1	REF:	32

	15.	ANS:	F	PTS:	1	REF:	35

MULTIPLE CHOICE

	16.	ANS:	A	PTS:	1	REF:	20

	17.	ANS:	B	PTS:	1	REF:	20

	18.	ANS:	B	PTS:	1	REF:	22

	19.	ANS:	C	PTS:	1	REF:	21

	20.	ANS:	D	PTS:	1	REF:	22

	21.	ANS:	C	PTS:	1	REF:	23

	22.	ANS:	A	PTS:	1	REF:	24

	23.	ANS:	D	PTS:	1	REF:	24

	24.	ANS:	B	PTS:	1	REF:	25

	25.	ANS:	C	PTS:	1	REF:	22

	26.	ANS:	A	PTS:	1	REF:	22

	27.	ANS:	A	PTS:	1	REF:	22

	28.	ANS:	D	PTS:	1	REF:	25

	29.	ANS:	B	PTS:	1	REF:	32-34

	30.	ANS:	A	PTS:	1	REF:	37

COMPLETION

	31.	ANS:	circuit

PTS:	1	REF:	20

	32.	ANS:	arithmetic

PTS:	1	REF:	21

	33.	ANS:	control

PTS:	1	REF:	22

	34.	ANS:	machine

PTS:	1	REF:	24

	35.	ANS:	cycle

PTS:	1	REF:	24

	36.	ANS:	cards

PTS:	1	REF:	29

	37.	ANS:	motherboard

PTS:	1	REF:	23

	38.	ANS:	
ASCII
American Standard Code for Information Interchange

PTS:	1	REF:	22

	39.	ANS:	
8
eight

PTS:	1	REF:	22

	40.	ANS:	expansion slot

PTS:	1	REF:	22

	41.	ANS:	modem

PTS:	1	REF:	25

	42.	ANS:	function

PTS:	1	REF:	26

	43.	ANS:	clicking

PTS:	1	REF:	27

	44.	ANS:	
printer
plotter

PTS:	1	REF:	32

	45.	ANS:	
hard disk drive
hard drive
hard disk

PTS:	1	REF:	36

	46.	ANS:	
Arrow
Directional

PTS:	1	REF:	26

	47.	ANS:	
pointer
mouse pointer

PTS:	1	REF:	27

	48.	ANS:	magnetic scanner

PTS:	1	REF:	28

	49.	ANS:	laser

PTS:	1	REF:	33

	50.	ANS:	magnetic tape drive

PTS:	1	REF:	36
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